025-0020 LED Roadbook lighting 60mm

contains:
1 x LED lighting strip
2 x scotchlock connectors
 
Drill a hole in the bottom of your Mini-roadbook housing large enough to squeeze the black rubber grommet in tightly.  Pass the wires thru the grommet and connect the red wire to the positive 12vDC supply.  Connect the black wire to the negative, or ground.  It is ideal if the red wire comes from a switched supply.

An ideal supply would be from the instrument lighting on the motorcycle but any switched source is good.  The power draw from this lighting is very, very low.  Secure the lighting to the back surface of the roadbook with double-stick tape.  Or Silicone works good too but prevent the circuitboard from touching the metal roadbook housing.

THESE INSTRUCTIONS ARE AT OUR PRESENT LEVEL OF KNOWLEDGE.  LEGAL REQUIREMENTS FOR CORRECTNESS DO NOT EXIST.  TECHNICAL ISSUES SUBJECT TO CHANGE.