030-0027 BMW Accessory Socket with 15A fuse

contains:

1 x electrical system plug socket pre-mounted
1 x steering wheel clip rubberized 22mm
1 x steering wheel clip rubberized 12mm
2 x zip-tie
2 x adapter female
2 x connecting cable (red and black)
1 x plastic tubing
2 x scotch-lock power taps
1 x 15A fuse
1 x Fuse Holder

The connection to the electrical system takes place by means of the two included wires in red and black. Optional to use the Scotchlocks to tap into existing 12v+ and ground wires.  Decide whether you want the outlet to be switched by the key, or direct to the battery (continuous). The ground connection can be direct to the battery in all cases. The plastic tubing is provided as an option to protect the lines against damage. The electrical system plug socket can be fastened with the large handlebar loop (for Ø 22mm = 7/8"), or onto a Ø 12mm crossbar with the smaller loop.

NOTE: Masseanschluss = GROUND.  The center terminal is the +12V.

Insert the 15A fuse into the fuse holder as the last step.

THESE INSTRUCTIONS ARE AT OUR PRESENT LEVEL OF KNOWLEDGE.  LEGAL REQUIREMENTS FOR CORRECTNESS DO NOT EXIST.  TECHNICAL ISSUES SUBJECT TO CHANGE.