055-1062 TOURATECH VP45 Tankbag
ENGLISH translation (text ONLY): http://www.touratech-usa.com/docs/09-055-1062-1.rtf

Please see German Instructions for photos: http://www.touratech.de/shop/media/09-055-1062-0.pdf

Parts included:
........

INSTALLATION INSTRUCTIONS:

!!!!!!!   Not yet translated.
!!!!!!!   Basic assistance only:

The fuel filler hole on the tankbag base as supplied is not cutout.  There is a circle sewn that shows the location of the R11xxGS filler cap.

First, cut a small hole about 2 inch diameter in the center of the sewn circle.  Place the baseplate on the motorcycle and verify that it is where you want the hole.  Typically if you cut just inside the sewn circle (about 1/4 inch) it will fit perfectly.

The sidepanniers have tie-down straps at the bottom.  If you have crashbars, attach then top the crashbars, but be careful that they cannot slide and touch the exhaust.  If no crashbars, they are attached together left to right BELOW the telelever suspension arm.  Do this with the bike on the centerstand and front tire off the ground.

The front straps wrap around the front fairing.  The rear straps simply attach around the motorcycle frame under the seat.