370-0132 LC8 Skid plate Tool Box

Contains:
1 x tool box with lock
2 x M6x20 countersunk screw
2 x M6x16 domehead screw
6 x M6 washer large
2 x M6 washer small
4 x M6 nylock nut

Installation:
Removing the tool box lid makes installation a bit easier and if you attach it again after reinstalling the skid plate on your bike.

Remove the skid plate attachment bolts and remove the skid plate off the bike.  Remove the two screws under the large holes and the LC8 logo on the front of the skid plate.

Attach the tool box with the two M6x20 screws, M6 washers small outside, M6 washers large outside and M6 nylock nuts on the points below the large holes and the LC8 logo on the front of the skid plate.

Attach the tool box on the bottom with two M6x16 domehead screws, M6 two washers large each and M6 nylock nuts.

These instructions are at our current level of knowledge.  Legal requirements do not exist.  Technical issues subject to change.