055-1088 LC4 VP45 Tankbag

1) Installation of the base plate.  The rear straps will be attached around the frame rails on both sides under the tank.  Make sure the straps are put through the buckles correctly.

2) Installation of the base plate front straps.  The front left & right straps are used for the front attachment for example around the cockpit fairing support brace.

3) The soft side panniers are attached to the base plate with the heavy-duty zippers.  The straps can be attached on the tank support as shown on photo 3.

4) The tankbag is attached on the base plate with the heavy duty zipper.

5)  The tankbag can be extended by opening the other zipper all around the bag.  The height is extended by about 10cm or 4".

for 4+5)  The clear map holder is easy to put on and take off with the velcro attachment.  Put it on and take it off few times when you first use the bag.  This helps the velcro to attach tighter.

6) The map holder can also be used without the tank by just attaching it on the base plate.

7) Conversion to back bag can be done with the two supplied straps by attaching them on the top as well as bottom corners as shown on photo 6.

8) Make sure the complete tankbag assembly is tightly fitted on your bike prior to each ride!

9)  Rain cover is also available for the tankbag part (055-0069)